**Toilet attachments with a cover AT51201, AT51202** are intended for people with arthritis,

people after hip surgery, and others who have difficulty moving,

standing up and sitting down. The cap has a modern mounting system that allows

easy to stabilize on the toilet. Ergonomically designed cap surface

causes an even distribution of pressure forces on the user's body surface. Light

seat angle inclination promotes correct posture and reduces joint flexion

hip and knee. The toilet cap has two cutouts on the front and

rear, which make it easier to perform hygienic activities in a sitting position.

Product characteristics:

• two fixing tabs adapt to the toilet bowl

• the attachment of the cap is simple, just tighten the two hooks

• The product is available in 2 heights: 10 and 15 cm

The attachments are comfortable and ergonomic:

• profiled upper surface of the cap is adapted to the shape of the body

• large front and rear support surface

DIMENSIONS (width x length): 40 x 36 cm

Maximum user weight: 180 kg

Product weight: AT51201 - 1.2 kg, AT51202 - 1.4 kg

FUNCTIONALITY:

• large cutouts at the front and back facilitate intimate hygiene

• opening the lid without touching the seat

• possibility to sit down with the lid down

CLEANING:

• Easy to clean, free from rough external surfaces

• Do not use abrasive or scouring cleaners.

• If there are any defects or damage, notify immediately

about this supplier. Do not use the product if you suspect that it is damaged or

some parts are missing.

• Clean with hot soapy water or a mild detergent

When a product related "serious incident" occurs, either directly or indirectly

led, could lead, or could lead to any of the following

events:

a) death of a health condition of a patient, user or other person, or

(b) temporary or permanent deterioration in the health of a patient, user or other person, or

c) a serious threat to public health

the above "serious incident" should be reported to the producer and the competent state authority

the state in which the user or patient resides. In the case of Poland

the competent authority is the Office for Registration of Medicinal Products, Medical Devices and Products

Biocidal.

CAUTION:

In case of pain, allergic reactions or other disturbing reactions that are not clear to the user

symptoms related to the use of a medical device, consult a service employee

health.

METHOD OF DISPOSAL OF THE PRODUCT AFTER REMOVING FROM SERVICE

After the device is withdrawn from use, the medical device can be disposed of as normal municipal waste, except for devices

electrical equipment - proceed in the manner appropriate for the disposal of electrical and electronic equipment.

Assembly:

• Place the front part of the cap on the front part of the toilet, and then screw them on

fastenings with side screws. Ergonomic and solid construction of the screws enables

accurate and permanent immobilization of the cap. The mounts have been secured against

the possibility of sliding.

Both the raised and lowered cover is protected against accidental operation

disassembly.

COMMENTS

1. During use and when folding and adjusting the mechanisms may

there is a risk of entrapment and / or pinching of body parts of the user / person

accompanying in openings / gaps between elements.

2. After completing the adjustment, stabilize the position by tightening the nuts /

screws.

3. Before each use of the product, always check that all

the adjustable parts are fixed well.

4. Use caution on wet or slippery surfaces.

5. Do not put your fingers into the drainage holes in the seat. It threatens

it trims or gets your finger caught.

6. Do not use a defective or broken cap.

7. Keep the product away from children. The maximum load does not apply to the cover.

8. The cover is not intended for sitting

9. The booster attachment is not intended to be used continuously on it.

10. Parts of clothing or body may be pinched when the armrests are lowered

11. Missing, damaged or worn parts may only be replaced by an authorized service center

12. Do not use high-pressure cleaners or aggressive, caustic cleaners for cleaning.